Adjusted for backport to c8s by modifying sysdeps/x86/cacheinfo.h.

commit 885a7f0feee951f514a121788f46f33b2867110f
Author: Noah Goldstein <goldstein.w.n@gmail.com>
Date:   Fri Aug 11 12:29:11 2023 -0500

    x86: Fix incorrect scope of setting `shared_per_thread` [BZ# 30745]
    
    The:
    
    ```
        if (shared_per_thread > 0 && threads > 0)
          shared_per_thread /= threads;
    ```
    
    Code was accidentally moved to inside the else scope.  This doesn't
    match how it was previously (before af992e7abd).
    
    This patch fixes that by putting the division after the `else` block.

diff --git a/sysdeps/x86/cacheinfo.h b/sysdeps/x86/cacheinfo.h
index 4dbfa979ef052eaa..e53fa25106c95253 100644
--- a/sysdeps/x86/cacheinfo.h
+++ b/sysdeps/x86/cacheinfo.h
@@ -243,11 +243,10 @@ get_common_cache_info (long int *shared_ptr, long int * shared_per_thread_ptr, u
 	     level.  */
 	  threads = ((cpu_features->features[COMMON_CPUID_INDEX_1].cpuid.ebx >> 16)
 		     & 0xff);
-
-	  /* Get per-thread size of highest level cache.  */
-	  if (shared_per_thread > 0 && threads > 0)
-	    shared_per_thread /= threads;
 	}
+      /* Get per-thread size of highest level cache.  */
+      if (shared_per_thread > 0 && threads > 0)
+	shared_per_thread /= threads;
     }
 
   /* Account for non-inclusive L2 and L3 caches.  */
