From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Daniel Axtens <dja@axtens.net>
Date: Tue, 8 Mar 2022 18:17:03 +1100
Subject: [PATCH] net/http: Fix OOB write for split http headers

GRUB has special code for handling an http header that is split
across two packets.

The code tracks the end of line by looking for a "\n" byte. The
code for split headers has always advanced the pointer just past the
end of the line, whereas the code that handles unsplit headers does
not advance the pointer. This extra advance causes the length to be
one greater, which breaks an assumption in parse_line(), leading to
it writing a NUL byte one byte past the end of the buffer where we
reconstruct the line from the two packets.

It's conceivable that an attacker controlled set of packets could
cause this to zero out the first byte of the "next" pointer of the
grub_mm_region structure following the current_line buffer.

Do not advance the pointer in the split header case.

Fixes: CVE-2022-28734

Signed-off-by: Daniel Axtens <dja@axtens.net>
Reviewed-by: Daniel Kiper <daniel.kiper@oracle.com>
(cherry picked from commit e9fb459638811c12b0989dbf64e3e124974ef617)
(cherry picked from commit b604916beb6c39e8ed27f72851eb16f3eaa293c5)
(cherry picked from commit c3c6b1167a43275991efd6847160a46ce3839fae)
---
 grub-core/net/http.c | 4 +---
 1 file changed, 1 insertion(+), 3 deletions(-)

diff --git a/grub-core/net/http.c b/grub-core/net/http.c
index 5223ca57a4..7fa2dcaea7 100644
--- a/grub-core/net/http.c
+++ b/grub-core/net/http.c
@@ -193,9 +193,7 @@ http_receive (grub_net_tcp_socket_t sock __attribute__ ((unused)),
 	  int have_line = 1;
 	  char *t;
 	  ptr = grub_memchr (nb->data, '\n', nb->tail - nb->data);
-	  if (ptr)
-	    ptr++;
-	  else
+	  if (ptr == NULL)
 	    {
 	      have_line = 0;
 	      ptr = (char *) nb->tail;
