From 5c3f4066462a5f6cac04d3dd81c9f551fabbc6c7 Mon Sep 17 00:00:00 2001
From: Keith Busch <kbusch@kernel.org>
Date: Thu, 12 Oct 2023 11:13:51 -0700
Subject: [PATCH] nvme-pci: add BOGUS_NID for Intel 0a54 device

These ones claim cmic and nmic capable, so need special consideration to ignore
their duplicate identifiers.

Link: https://bugzilla.kernel.org/show_bug.cgi?id=217981
Reported-by: welsh@cassens.com
Signed-off-by: Keith Busch <kbusch@kernel.org>
---
 drivers/nvme/host/pci.c | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

diff --git a/drivers/nvme/host/pci.c b/drivers/nvme/host/pci.c
index 347cb5daebc3..3f0c9ee09a12 100644
--- a/drivers/nvme/host/pci.c
+++ b/drivers/nvme/host/pci.c
@@ -3329,7 +3329,8 @@ static const struct pci_device_id nvme_id_table[] = {
 	{ PCI_VDEVICE(INTEL, 0x0a54),	/* Intel P4500/P4600 */
 		.driver_data = NVME_QUIRK_STRIPE_SIZE |
 				NVME_QUIRK_DEALLOCATE_ZEROES |
-				NVME_QUIRK_IGNORE_DEV_SUBNQN, },
+				NVME_QUIRK_IGNORE_DEV_SUBNQN |
+				NVME_QUIRK_BOGUS_NID, },
 	{ PCI_VDEVICE(INTEL, 0x0a55),	/* Dell Express Flash P4600 */
 		.driver_data = NVME_QUIRK_STRIPE_SIZE |
 				NVME_QUIRK_DEALLOCATE_ZEROES, },
-- 
2.27.0

