From e3a1c2ff0d7b930b1782d59d093fd15471d3aee1 Mon Sep 17 00:00:00 2001
From: "plai@redhat.com" <plai@redhat.com>
Date: Thu, 21 May 2020 23:56:46 +0100
Subject: [PATCH 03/12] numa: properly check if numa is supported

RH-Author: plai@redhat.com
Message-id: <20200521235655.27141-3-plai@redhat.com>
Patchwork-id: 96732
O-Subject: [RHEL8.2.1 AV qemu-kvm PATCH 02/11] numa: properly check if numa is supported
Bugzilla: 1600217
RH-Acked-by: Michael S. Tsirkin <mst@redhat.com>
RH-Acked-by: Igor Mammedov <imammedo@redhat.com>
RH-Acked-by: Eduardo Habkost <ehabkost@redhat.com>

From: Igor Mammedov <imammedo@redhat.com>

Commit aa57020774b, by mistake used MachineClass::numa_mem_supported
to check if NUMA is supported by machine and also as unrelated change
set it to true for sbsa-ref board.

Luckily change didn't break machines that support NUMA, as the field
is set to true for them.

But the field is not intended for checking if NUMA is supported and
will be flipped to false within this release for new machine types.

Fix it:
 - by using previously used condition
      !mc->cpu_index_to_instance_props || !mc->get_default_cpu_node_id
   the first time and then use MachineState::numa_state down the road
   to check if NUMA is supported
 - dropping stray sbsa-ref chunk

Fixes: aa57020774b690a22be72453b8e91c9b5a68c516
Signed-off-by: Igor Mammedov <imammedo@redhat.com>
Message-Id: <1576154936-178362-3-git-send-email-imammedo@redhat.com>
Signed-off-by: Eduardo Habkost <ehabkost@redhat.com>
(cherry picked from commit fcd3f2cc124600385dba46c69a80626985c15b50)
Signed-off-by: Danilo C. L. de Paula <ddepaula@redhat.com>
---
 hw/arm/sbsa-ref.c | 1 -
 hw/core/machine.c | 4 ++--
 2 files changed, 2 insertions(+), 3 deletions(-)

diff --git a/hw/arm/sbsa-ref.c b/hw/arm/sbsa-ref.c
index 27046cc..c6261d4 100644
--- a/hw/arm/sbsa-ref.c
+++ b/hw/arm/sbsa-ref.c
@@ -791,7 +791,6 @@ static void sbsa_ref_class_init(ObjectClass *oc, void *data)
     mc->possible_cpu_arch_ids = sbsa_ref_possible_cpu_arch_ids;
     mc->cpu_index_to_instance_props = sbsa_ref_cpu_index_to_props;
     mc->get_default_cpu_node_id = sbsa_ref_get_default_cpu_node_id;
-    mc->numa_mem_supported = true;
 }
 
 static const TypeInfo sbsa_ref_info = {
diff --git a/hw/core/machine.c b/hw/core/machine.c
index 5a025d1..19c78c6 100644
--- a/hw/core/machine.c
+++ b/hw/core/machine.c
@@ -1128,7 +1128,7 @@ static void machine_initfn(Object *obj)
                                         NULL);
     }
 
-    if (mc->numa_mem_supported) {
+    if (mc->cpu_index_to_instance_props && mc->get_default_cpu_node_id) {
         ms->numa_state = g_new0(NumaState, 1);
     }
 
@@ -1272,7 +1272,7 @@ void machine_run_board_init(MachineState *machine)
 {
     MachineClass *machine_class = MACHINE_GET_CLASS(machine);
 
-    if (machine_class->numa_mem_supported) {
+    if (machine->numa_state) {
         numa_complete_configuration(machine);
         if (machine->numa_state->num_nodes) {
             machine_numa_finish_cpu_init(machine);
-- 
1.8.3.1

