From 113078b23a4747b07eb363719d7cbc0af403dd2a Mon Sep 17 00:00:00 2001
From: Miroslav Rezanina <mrezanin@redhat.com>
Date: Fri, 11 Jan 2019 09:54:45 +0100
Subject: Machine type related general changes

This patch is first part of original "Add RHEL machine types" patch we
split to allow easier review. It contains changes not related to any
architecture.

Signed-off-by: Miroslav Rezanina <mrezanin@redhat.com>

Rebase changes (4.0.0):
- Remove e1000 device duplication changes to reflect upstream solution
- Rewrite machine compat properties to upstream solution

Rebase changes (4.1.0):
- Removed optional flag for machine compat properties (upstream)
- Remove c3e002cb chunk from hw/net/e1000.c
- Reorder compat structures
- Use one format for compat scructures
- Added compat for virtio-balloon-pci.any_layout for rhel71

Merged patches (4.0.0):
- d4c0957 compat: Generic HW_COMPAT_RHEL7_6
- cbac773 virtio: Make disable-legacy/disable-modern compat properties optional

Merged patches (4.1.0):
- 479ad30 redhat: fix cut'n'paste garbage in hw_compat comments
- f19738e compat: Generic hw_compat_rhel_8_0

Merged patches (4.2.0):
- 9f2bfaa machine types: Update hw_compat_rhel_8_0 from hw_compat_4_0
- ca4a5e8 virtio: Make disable-legacy/disable-modern compat properties optional
- compat: Generic hw_compat_rhel_8_1 (patch 93040/92956)

Signed-off-by: Danilo C. L. de Paula <ddepaula@redhat.com>
---
 hw/acpi/ich9.c          |  16 ++++
 hw/acpi/piix4.c         |   5 +-
 hw/char/serial.c        |  16 ++++
 hw/core/machine.c       | 170 ++++++++++++++++++++++++++++++++++++++++
 hw/display/vga-isa.c    |   2 +-
 hw/net/e1000e.c         |  21 +++++
 hw/net/rtl8139.c        |   4 +-
 hw/rtc/mc146818rtc.c    |   6 ++
 hw/smbios/smbios.c      |   1 +
 hw/timer/i8254_common.c |   2 +-
 hw/usb/hcd-uhci.c       |   4 +-
 hw/usb/hcd-xhci.c       |  20 +++++
 hw/usb/hcd-xhci.h       |   2 +
 include/hw/acpi/ich9.h  |   3 +
 include/hw/boards.h     |  24 ++++++
 include/hw/usb.h        |   4 +
 migration/migration.c   |   2 +
 migration/migration.h   |   5 ++
 18 files changed, 301 insertions(+), 6 deletions(-)

diff --git a/hw/acpi/ich9.c b/hw/acpi/ich9.c
index ab203ad448..7ec26884e8 100644
--- a/hw/acpi/ich9.c
+++ b/hw/acpi/ich9.c
@@ -444,6 +444,18 @@ static void ich9_pm_set_enable_tco(Object *obj, bool value, Error **errp)
     s->pm.enable_tco = value;
 }
 
+static bool ich9_pm_get_force_rev1_fadt(Object *obj, Error **errp)
+{
+    ICH9LPCState *s = ICH9_LPC_DEVICE(obj);
+    return s->pm.force_rev1_fadt;
+}
+
+static void ich9_pm_set_force_rev1_fadt(Object *obj, bool value, Error **errp)
+{
+    ICH9LPCState *s = ICH9_LPC_DEVICE(obj);
+    s->pm.force_rev1_fadt = value;
+}
+
 void ich9_pm_add_properties(Object *obj, ICH9LPCPMRegs *pm, Error **errp)
 {
     static const uint32_t gpe0_len = ICH9_PMIO_GPE0_LEN;
@@ -468,6 +480,10 @@ void ich9_pm_add_properties(Object *obj, ICH9LPCPMRegs *pm, Error **errp)
                              ich9_pm_get_cpu_hotplug_legacy,
                              ich9_pm_set_cpu_hotplug_legacy,
                              NULL);
+    object_property_add_bool(obj, "__com.redhat_force-rev1-fadt",
+                             ich9_pm_get_force_rev1_fadt,
+                             ich9_pm_set_force_rev1_fadt,
+                             NULL);
     object_property_add(obj, ACPI_PM_PROP_S3_DISABLED, "uint8",
                         ich9_pm_get_disable_s3,
                         ich9_pm_set_disable_s3,
diff --git a/hw/acpi/piix4.c b/hw/acpi/piix4.c
index 93aec2dd2c..3a26193cbe 100644
--- a/hw/acpi/piix4.c
+++ b/hw/acpi/piix4.c
@@ -274,6 +274,7 @@ static const VMStateDescription vmstate_acpi = {
     .name = "piix4_pm",
     .version_id = 3,
     .minimum_version_id = 3,
+    .minimum_version_id = 2,
     .post_load = vmstate_acpi_post_load,
     .fields = (VMStateField[]) {
         VMSTATE_PCI_DEVICE(parent_obj, PIIX4PMState),
@@ -627,8 +628,8 @@ static void piix4_send_gpe(AcpiDeviceIf *adev, AcpiEventStatusBits ev)
 
 static Property piix4_pm_properties[] = {
     DEFINE_PROP_UINT32("smb_io_base", PIIX4PMState, smb_io_base, 0),
-    DEFINE_PROP_UINT8(ACPI_PM_PROP_S3_DISABLED, PIIX4PMState, disable_s3, 0),
-    DEFINE_PROP_UINT8(ACPI_PM_PROP_S4_DISABLED, PIIX4PMState, disable_s4, 0),
+    DEFINE_PROP_UINT8(ACPI_PM_PROP_S3_DISABLED, PIIX4PMState, disable_s3, 1),
+    DEFINE_PROP_UINT8(ACPI_PM_PROP_S4_DISABLED, PIIX4PMState, disable_s4, 1),
     DEFINE_PROP_UINT8(ACPI_PM_PROP_S4_VAL, PIIX4PMState, s4_val, 2),
     DEFINE_PROP_BOOL("acpi-pci-hotplug-with-bridge-support", PIIX4PMState,
                      use_acpi_pci_hotplug, true),
diff --git a/hw/char/serial.c b/hw/char/serial.c
index b4aa250950..0012f0e44d 100644
--- a/hw/char/serial.c
+++ b/hw/char/serial.c
@@ -34,6 +34,7 @@
 #include "sysemu/runstate.h"
 #include "qemu/error-report.h"
 #include "trace.h"
+#include "migration/migration.h"
 
 //#define DEBUG_SERIAL
 
@@ -703,6 +704,9 @@ static int serial_post_load(void *opaque, int version_id)
 static bool serial_thr_ipending_needed(void *opaque)
 {
     SerialState *s = opaque;
+    if (migrate_pre_2_2) {
+        return false;
+    }
 
     if (s->ier & UART_IER_THRI) {
         bool expected_value = ((s->iir & UART_IIR_ID) == UART_IIR_THRI);
@@ -784,6 +788,10 @@ static const VMStateDescription vmstate_serial_xmit_fifo = {
 static bool serial_fifo_timeout_timer_needed(void *opaque)
 {
     SerialState *s = (SerialState *)opaque;
+    if (migrate_pre_2_2) {
+        return false;
+    }
+
     return timer_pending(s->fifo_timeout_timer);
 }
 
@@ -801,6 +809,10 @@ static const VMStateDescription vmstate_serial_fifo_timeout_timer = {
 static bool serial_timeout_ipending_needed(void *opaque)
 {
     SerialState *s = (SerialState *)opaque;
+    if (migrate_pre_2_2) {
+        return false;
+    }
+
     return s->timeout_ipending != 0;
 }
 
@@ -818,6 +830,10 @@ static const VMStateDescription vmstate_serial_timeout_ipending = {
 static bool serial_poll_needed(void *opaque)
 {
     SerialState *s = (SerialState *)opaque;
+    if (migrate_pre_2_2) {
+        return false;
+    }
+
     return s->poll_msl >= 0;
 }
 
diff --git a/hw/core/machine.c b/hw/core/machine.c
index 1689ad3bf8..e0e0eec8bf 100644
--- a/hw/core/machine.c
+++ b/hw/core/machine.c
@@ -27,6 +27,176 @@
 #include "hw/pci/pci.h"
 #include "hw/mem/nvdimm.h"
 
+/*
+ * The same as hw_compat_4_1
+ */
+GlobalProperty hw_compat_rhel_8_1[] = {
+    /* hw_compat_rhel_8_1 from hw_compat_4_1 */
+    { "virtio-pci", "x-pcie-flr-init", "off" },
+};
+const size_t hw_compat_rhel_8_1_len = G_N_ELEMENTS(hw_compat_rhel_8_1);
+
+/* The same as hw_compat_3_1
+ * format of array has been changed by:
+ *     6c36bddf5340 ("machine: Use shorter format for GlobalProperty arrays")
+ */
+GlobalProperty hw_compat_rhel_8_0[] = {
+    /* hw_compat_rhel_8_0 from hw_compat_3_1 */
+    { "pcie-root-port", "x-speed", "2_5" },
+    /* hw_compat_rhel_8_0 from hw_compat_3_1 */
+    { "pcie-root-port", "x-width", "1" },
+    /* hw_compat_rhel_8_0 from hw_compat_3_1 */
+    { "memory-backend-file", "x-use-canonical-path-for-ramblock-id", "true" },
+    /* hw_compat_rhel_8_0 from hw_compat_3_1 */
+    { "memory-backend-memfd", "x-use-canonical-path-for-ramblock-id", "true" },
+    /* hw_compat_rhel_8_0 from hw_compat_3_1 */
+    { "tpm-crb", "ppi", "false" },
+    /* hw_compat_rhel_8_0 from hw_compat_3_1 */
+    { "tpm-tis", "ppi", "false" },
+    /* hw_compat_rhel_8_0 from hw_compat_3_1 */
+    { "usb-kbd", "serial", "42" },
+    /* hw_compat_rhel_8_0 from hw_compat_3_1 */
+    { "usb-mouse", "serial", "42" },
+    /* hw_compat_rhel_8_0 from hw_compat_3_1 */
+    { "usb-tablet", "serial", "42" },
+    /* hw_compat_rhel_8_0 from hw_compat_3_1 */
+    { "virtio-blk-device", "discard", "false" },
+    /* hw_compat_rhel_8_0 from hw_compat_3_1 */
+    { "virtio-blk-device", "write-zeroes", "false" },
+    /* hw_compat_rhel_8_0 from hw_compat_4_0 */
+    { "VGA",            "edid", "false" },
+    /* hw_compat_rhel_8_0 from hw_compat_4_0 */
+    { "secondary-vga",  "edid", "false" },
+    /* hw_compat_rhel_8_0 from hw_compat_4_0 */
+    { "bochs-display",  "edid", "false" },
+    /* hw_compat_rhel_8_0 from hw_compat_4_0 */
+    { "virtio-vga",     "edid", "false" },
+    /* hw_compat_rhel_8_0 from hw_compat_4_0 */
+    { "virtio-gpu-pci", "edid", "false" },
+    /* hw_compat_rhel_8_0 from hw_compat_4_0 */
+    { "virtio-device", "use-started", "false" },
+    /* hw_compat_rhel_8_0 from hw_compat_3_1 - that was added in 4.1 */
+    { "pcie-root-port-base", "disable-acs", "true" },
+};
+const size_t hw_compat_rhel_8_0_len = G_N_ELEMENTS(hw_compat_rhel_8_0);
+
+/* The same as hw_compat_3_0 + hw_compat_2_12
+ * except that
+ *   there's nothing in 3_0
+ *   migration.decompress-error-check=off was in 7.5 from bz 1584139
+ */
+GlobalProperty hw_compat_rhel_7_6[] = {
+    /* hw_compat_rhel_7_6 from hw_compat_2_12 */
+    { "hda-audio", "use-timer", "false" },
+    /* hw_compat_rhel_7_6 from hw_compat_2_12 */
+    { "cirrus-vga", "global-vmstate", "true" },
+    /* hw_compat_rhel_7_6 from hw_compat_2_12 */
+    { "VGA", "global-vmstate", "true" },
+    /* hw_compat_rhel_7_6 from hw_compat_2_12 */
+    { "vmware-svga", "global-vmstate", "true" },
+    /* hw_compat_rhel_7_6 from hw_compat_2_12 */
+    { "qxl-vga", "global-vmstate",  "true" },
+};
+const size_t hw_compat_rhel_7_6_len = G_N_ELEMENTS(hw_compat_rhel_7_6);
+
+/* The same as hw_compat_2_11 + hw_compat_2_10 */
+GlobalProperty hw_compat_rhel_7_5[] = {
+    /* hw_compat_rhel_7_5 from hw_compat_2_11 */
+    { "hpet", "hpet-offset-saved", "false" },
+    /* hw_compat_rhel_7_5 from hw_compat_2_11 */
+    { "virtio-blk-pci", "vectors", "2" },
+    /* hw_compat_rhel_7_5 from hw_compat_2_11 */
+    { "vhost-user-blk-pci", "vectors", "2" },
+    /* hw_compat_rhel_7_5 from hw_compat_2_11
+       bz 1608778 modified for our naming */
+    { "e1000-82540em", "migrate_tso_props", "off" },
+    /* hw_compat_rhel_7_5 from hw_compat_2_10 */
+    { "virtio-mouse-device", "wheel-axis", "false" },
+    /* hw_compat_rhel_7_5 from hw_compat_2_10 */
+    { "virtio-tablet-device", "wheel-axis", "false" },
+    { "cirrus-vga", "vgamem_mb", "16" },
+    { "migration", "decompress-error-check", "off" },
+};
+const size_t hw_compat_rhel_7_5_len = G_N_ELEMENTS(hw_compat_rhel_7_5);
+
+/* Mostly like hw_compat_2_9 except
+ * x-mtu-bypass-backend, x-migrate-msix has already been
+ * backported to RHEL7.4. shpc was already on in 7.4.
+ */
+GlobalProperty hw_compat_rhel_7_4[] = {
+    { "intel-iommu", "pt", "off" },
+};
+
+const size_t hw_compat_rhel_7_4_len = G_N_ELEMENTS(hw_compat_rhel_7_4);
+/* Mostly like HW_COMPAT_2_6 + HW_COMPAT_2_7 + HW_COMPAT_2_8 except
+ * disable-modern, disable-legacy, page-per-vq have already been
+ * backported to RHEL7.3
+ */
+GlobalProperty hw_compat_rhel_7_3[] = {
+    { "virtio-mmio", "format_transport_address", "off" },
+    { "virtio-serial-device", "emergency-write", "off" },
+    { "ioapic", "version", "0x11" },
+    { "intel-iommu", "x-buggy-eim", "true" },
+    { "virtio-pci", "x-ignore-backend-features", "on" },
+    { "fw_cfg_mem", "x-file-slots", stringify(0x10) },
+    { "fw_cfg_io", "x-file-slots", stringify(0x10) },
+    { "pflash_cfi01", "old-multiple-chip-handling", "on" },
+    { TYPE_PCI_DEVICE, "x-pcie-extcap-init", "off" },
+    { "virtio-pci", "x-pcie-deverr-init", "off" },
+    { "virtio-pci", "x-pcie-lnkctl-init", "off" },
+    { "virtio-pci", "x-pcie-pm-init", "off" },
+    { "virtio-net-device", "x-mtu-bypass-backend", "off" },
+    { "e1000e", "__redhat_e1000e_7_3_intr_state", "on" },
+};
+const size_t hw_compat_rhel_7_3_len = G_N_ELEMENTS(hw_compat_rhel_7_3);
+
+/* Mostly like hw_compat_2_4 + 2_3 but:
+ *  we don't need "any_layout" as it has been backported to 7.2
+ */
+GlobalProperty hw_compat_rhel_7_2[] = {
+        { "virtio-blk-device", "scsi", "true" },
+        { "e1000-82540em", "extra_mac_registers", "off" },
+        { "virtio-pci", "x-disable-pcie", "on" },
+        { "virtio-pci", "migrate-extra", "off" },
+        { "fw_cfg_mem", "dma_enabled", "off" },
+        { "fw_cfg_io", "dma_enabled", "off" },
+        { "isa-fdc", "fallback", "144" },
+        /* Optional because not all virtio-pci devices support legacy mode */
+        { "virtio-pci", "disable-modern", "on", .optional = true },
+        { "virtio-pci", "disable-legacy", "off", .optional = true },
+        { TYPE_PCI_DEVICE, "x-pcie-lnksta-dllla", "off" },
+        { "virtio-pci", "page-per-vq", "on" },
+        /* hw_compat_rhel_7_2 - introduced with 2.10.0 */
+        { "migration", "send-section-footer", "off" },
+        /* hw_compat_rhel_7_2 - introduced with 2.10.0 */
+        { "migration", "store-global-state", "off",
+        },
+};
+const size_t hw_compat_rhel_7_2_len = G_N_ELEMENTS(hw_compat_rhel_7_2);
+
+/* Mostly like hw_compat_2_1 but:
+ *    we don't need virtio-scsi-pci since 7.0 already had that on
+ *
+ * RH: Note, qemu-extended-regs should have been enabled in the 7.1
+ * machine type, but was accidentally turned off in 7.2 onwards.
+ */
+GlobalProperty hw_compat_rhel_7_1[] = {
+    { "intel-hda-generic", "old_msi_addr", "on" },
+    { "VGA", "qemu-extended-regs", "off" },
+    { "secondary-vga", "qemu-extended-regs", "off" },
+    { "usb-mouse", "usb_version", stringify(1) },
+    { "usb-kbd", "usb_version", stringify(1) },
+    { "virtio-pci",  "virtio-pci-bus-master-bug-migration", "on" },
+    { "virtio-blk-pci", "any_layout", "off" },
+    { "virtio-balloon-pci", "any_layout", "off" },
+    { "virtio-serial-pci", "any_layout", "off" },
+    { "virtio-9p-pci", "any_layout", "off" },
+    { "virtio-rng-pci", "any_layout", "off" },
+    /* HW_COMPAT_RHEL7_1 - introduced with 2.10.0 */
+    { "migration", "send-configuration", "off" },
+};
+const size_t hw_compat_rhel_7_1_len = G_N_ELEMENTS(hw_compat_rhel_7_1);
+
 GlobalProperty hw_compat_4_1[] = {
     { "virtio-pci", "x-pcie-flr-init", "off" },
 };
diff --git a/hw/display/vga-isa.c b/hw/display/vga-isa.c
index 873e5e9706..d1a2efe47e 100644
--- a/hw/display/vga-isa.c
+++ b/hw/display/vga-isa.c
@@ -82,7 +82,7 @@ static void vga_isa_realizefn(DeviceState *dev, Error **errp)
 }
 
 static Property vga_isa_properties[] = {
-    DEFINE_PROP_UINT32("vgamem_mb", ISAVGAState, state.vram_size_mb, 8),
+    DEFINE_PROP_UINT32("vgamem_mb", ISAVGAState, state.vram_size_mb, 16),
     DEFINE_PROP_END_OF_LIST(),
 };
 
diff --git a/hw/net/e1000e.c b/hw/net/e1000e.c
index b69fd7d8ad..d8be50a1ce 100644
--- a/hw/net/e1000e.c
+++ b/hw/net/e1000e.c
@@ -79,6 +79,11 @@ typedef struct E1000EState {
 
     E1000ECore core;
 
+    /* 7.3 had the intr_state field that was in the original e1000e code
+     * but that was removed prior to 2.7's release
+     */
+    bool redhat_7_3_intr_state_enable;
+    uint32_t redhat_7_3_intr_state;
 } E1000EState;
 
 #define E1000E_MMIO_IDX     0
@@ -94,6 +99,10 @@ typedef struct E1000EState {
 #define E1000E_MSIX_TABLE   (0x0000)
 #define E1000E_MSIX_PBA     (0x2000)
 
+/* Values as in RHEL 7.3 build and original upstream */
+#define RH_E1000E_USE_MSI     BIT(0)
+#define RH_E1000E_USE_MSIX    BIT(1)
+
 static uint64_t
 e1000e_mmio_read(void *opaque, hwaddr addr, unsigned size)
 {
@@ -305,6 +314,8 @@ e1000e_init_msix(E1000EState *s)
     } else {
         if (!e1000e_use_msix_vectors(s, E1000E_MSIX_VEC_NUM)) {
             msix_uninit(d, &s->msix, &s->msix);
+        } else {
+            s->redhat_7_3_intr_state |= RH_E1000E_USE_MSIX;
         }
     }
 }
@@ -476,6 +487,8 @@ static void e1000e_pci_realize(PCIDevice *pci_dev, Error **errp)
     ret = msi_init(PCI_DEVICE(s), 0xD0, 1, true, false, NULL);
     if (ret) {
         trace_e1000e_msi_init_fail(ret);
+    } else {
+        s->redhat_7_3_intr_state |= RH_E1000E_USE_MSI;
     }
 
     if (e1000e_add_pm_capability(pci_dev, e1000e_pmrb_offset,
@@ -599,6 +612,11 @@ static const VMStateDescription e1000e_vmstate_intr_timer = {
     VMSTATE_STRUCT_ARRAY(_f, _s, _num, 0,                           \
                          e1000e_vmstate_intr_timer, E1000IntrDelayTimer)
 
+static bool rhel_7_3_check(void *opaque, int version_id)
+{
+    return ((E1000EState *)opaque)->redhat_7_3_intr_state_enable;
+}
+
 static const VMStateDescription e1000e_vmstate = {
     .name = "e1000e",
     .version_id = 1,
@@ -610,6 +628,7 @@ static const VMStateDescription e1000e_vmstate = {
         VMSTATE_MSIX(parent_obj, E1000EState),
 
         VMSTATE_UINT32(ioaddr, E1000EState),
+        VMSTATE_UINT32_TEST(redhat_7_3_intr_state, E1000EState, rhel_7_3_check),
         VMSTATE_UINT32(core.rxbuf_min_shift, E1000EState),
         VMSTATE_UINT8(core.rx_desc_len, E1000EState),
         VMSTATE_UINT32_ARRAY(core.rxbuf_sizes, E1000EState,
@@ -658,6 +677,8 @@ static PropertyInfo e1000e_prop_disable_vnet,
 
 static Property e1000e_properties[] = {
     DEFINE_NIC_PROPERTIES(E1000EState, conf),
+    DEFINE_PROP_BOOL("__redhat_e1000e_7_3_intr_state", E1000EState,
+                        redhat_7_3_intr_state_enable, false),
     DEFINE_PROP_SIGNED("disable_vnet_hdr", E1000EState, disable_vnet, false,
                         e1000e_prop_disable_vnet, bool),
     DEFINE_PROP_SIGNED("subsys_ven", E1000EState, subsys_ven,
diff --git a/hw/net/rtl8139.c b/hw/net/rtl8139.c
index 88a97d756d..21d80e96cf 100644
--- a/hw/net/rtl8139.c
+++ b/hw/net/rtl8139.c
@@ -3177,7 +3177,7 @@ static int rtl8139_pre_save(void *opaque)
 
 static const VMStateDescription vmstate_rtl8139 = {
     .name = "rtl8139",
-    .version_id = 5,
+    .version_id = 4,
     .minimum_version_id = 3,
     .post_load = rtl8139_post_load,
     .pre_save  = rtl8139_pre_save,
@@ -3258,7 +3258,9 @@ static const VMStateDescription vmstate_rtl8139 = {
         VMSTATE_UINT32(tally_counters.TxMCol, RTL8139State),
         VMSTATE_UINT64(tally_counters.RxOkPhy, RTL8139State),
         VMSTATE_UINT64(tally_counters.RxOkBrd, RTL8139State),
+#if 0 /* Disabled for Red Hat Enterprise Linux bz 1420195 */
         VMSTATE_UINT32_V(tally_counters.RxOkMul, RTL8139State, 5),
+#endif
         VMSTATE_UINT16(tally_counters.TxAbt, RTL8139State),
         VMSTATE_UINT16(tally_counters.TxUndrn, RTL8139State),
 
diff --git a/hw/rtc/mc146818rtc.c b/hw/rtc/mc146818rtc.c
index 74ae74bc5c..73820517df 100644
--- a/hw/rtc/mc146818rtc.c
+++ b/hw/rtc/mc146818rtc.c
@@ -42,6 +42,7 @@
 #include "qapi/visitor.h"
 #include "exec/address-spaces.h"
 #include "hw/rtc/mc146818rtc_regs.h"
+#include "migration/migration.h"
 
 #ifdef TARGET_I386
 #include "qapi/qapi-commands-misc-target.h"
@@ -820,6 +821,11 @@ static int rtc_post_load(void *opaque, int version_id)
 static bool rtc_irq_reinject_on_ack_count_needed(void *opaque)
 {
     RTCState *s = (RTCState *)opaque;
+
+    if (migrate_pre_2_2) {
+        return false;
+    }
+
     return s->irq_reinject_on_ack_count != 0;
 }
 
diff --git a/hw/smbios/smbios.c b/hw/smbios/smbios.c
index 11d476c4a2..e6e9355384 100644
--- a/hw/smbios/smbios.c
+++ b/hw/smbios/smbios.c
@@ -777,6 +777,7 @@ void smbios_set_defaults(const char *manufacturer, const char *product,
     SMBIOS_SET_DEFAULT(type1.manufacturer, manufacturer);
     SMBIOS_SET_DEFAULT(type1.product, product);
     SMBIOS_SET_DEFAULT(type1.version, version);
+    SMBIOS_SET_DEFAULT(type1.family, "Red Hat Enterprise Linux");
     SMBIOS_SET_DEFAULT(type2.manufacturer, manufacturer);
     SMBIOS_SET_DEFAULT(type2.product, product);
     SMBIOS_SET_DEFAULT(type2.version, version);
diff --git a/hw/timer/i8254_common.c b/hw/timer/i8254_common.c
index 050875b497..32935da46c 100644
--- a/hw/timer/i8254_common.c
+++ b/hw/timer/i8254_common.c
@@ -231,7 +231,7 @@ static const VMStateDescription vmstate_pit_common = {
     .pre_save = pit_dispatch_pre_save,
     .post_load = pit_dispatch_post_load,
     .fields = (VMStateField[]) {
-        VMSTATE_UINT32_V(channels[0].irq_disabled, PITCommonState, 3),
+        VMSTATE_UINT32(channels[0].irq_disabled, PITCommonState), /* qemu-kvm's v2 had 'flags' here */
         VMSTATE_STRUCT_ARRAY(channels, PITCommonState, 3, 2,
                              vmstate_pit_channel, PITChannelState),
         VMSTATE_INT64(channels[0].next_transition_time,
diff --git a/hw/usb/hcd-uhci.c b/hw/usb/hcd-uhci.c
index 23507ad3b5..9fd87a7ad9 100644
--- a/hw/usb/hcd-uhci.c
+++ b/hw/usb/hcd-uhci.c
@@ -1219,12 +1219,14 @@ static void usb_uhci_common_realize(PCIDevice *dev, Error **errp)
     UHCIState *s = UHCI(dev);
     uint8_t *pci_conf = s->dev.config;
     int i;
+    int irq_pin;
 
     pci_conf[PCI_CLASS_PROG] = 0x00;
     /* TODO: reset value should be 0. */
     pci_conf[USB_SBRN] = USB_RELEASE_1; // release number
 
-    pci_config_set_interrupt_pin(pci_conf, u->info.irq_pin + 1);
+    irq_pin = u->info.irq_pin;
+    pci_config_set_interrupt_pin(pci_conf, irq_pin + 1);
 
     if (s->masterbus) {
         USBPort *ports[NB_PORTS];
diff --git a/hw/usb/hcd-xhci.c b/hw/usb/hcd-xhci.c
index 80988bb305..8fed2eedd6 100644
--- a/hw/usb/hcd-xhci.c
+++ b/hw/usb/hcd-xhci.c
@@ -3590,9 +3590,27 @@ static const VMStateDescription vmstate_xhci_slot = {
     }
 };
 
+static int xhci_event_pre_save(void *opaque)
+{
+    XHCIEvent *s = opaque;
+
+    s->cve_2014_5263_a = ((uint8_t *)&s->type)[0];
+    s->cve_2014_5263_b = ((uint8_t *)&s->type)[1];
+
+    return 0;
+}
+
+bool migrate_cve_2014_5263_xhci_fields;
+
+static bool xhci_event_cve_2014_5263(void *opaque, int version_id)
+{
+    return migrate_cve_2014_5263_xhci_fields;
+}
+
 static const VMStateDescription vmstate_xhci_event = {
     .name = "xhci-event",
     .version_id = 1,
+    .pre_save = xhci_event_pre_save,
     .fields = (VMStateField[]) {
         VMSTATE_UINT32(type,   XHCIEvent),
         VMSTATE_UINT32(ccode,  XHCIEvent),
@@ -3601,6 +3619,8 @@ static const VMStateDescription vmstate_xhci_event = {
         VMSTATE_UINT32(flags,  XHCIEvent),
         VMSTATE_UINT8(slotid,  XHCIEvent),
         VMSTATE_UINT8(epid,    XHCIEvent),
+        VMSTATE_UINT8_TEST(cve_2014_5263_a, XHCIEvent, xhci_event_cve_2014_5263),
+        VMSTATE_UINT8_TEST(cve_2014_5263_b, XHCIEvent, xhci_event_cve_2014_5263),
         VMSTATE_END_OF_LIST()
     }
 };
diff --git a/hw/usb/hcd-xhci.h b/hw/usb/hcd-xhci.h
index 2fad4df2a7..f554b671e3 100644
--- a/hw/usb/hcd-xhci.h
+++ b/hw/usb/hcd-xhci.h
@@ -157,6 +157,8 @@ typedef struct XHCIEvent {
     uint32_t flags;
     uint8_t slotid;
     uint8_t epid;
+    uint8_t cve_2014_5263_a;
+    uint8_t cve_2014_5263_b;
 } XHCIEvent;
 
 typedef struct XHCIInterrupter {
diff --git a/include/hw/acpi/ich9.h b/include/hw/acpi/ich9.h
index 41568d1837..1a23ccc412 100644
--- a/include/hw/acpi/ich9.h
+++ b/include/hw/acpi/ich9.h
@@ -61,6 +61,9 @@ typedef struct ICH9LPCPMRegs {
     uint8_t smm_enabled;
     bool enable_tco;
     TCOIORegs tco_regs;
+
+    /* RH addition, see bz 1489800 */
+    bool force_rev1_fadt;
 } ICH9LPCPMRegs;
 
 #define ACPI_PM_PROP_TCO_ENABLED "enable_tco"
diff --git a/include/hw/boards.h b/include/hw/boards.h
index de45087f34..6f85a0e032 100644
--- a/include/hw/boards.h
+++ b/include/hw/boards.h
@@ -377,4 +377,28 @@ extern const size_t hw_compat_2_2_len;
 extern GlobalProperty hw_compat_2_1[];
 extern const size_t hw_compat_2_1_len;
 
+extern GlobalProperty hw_compat_rhel_8_1[];
+extern const size_t hw_compat_rhel_8_1_len;
+
+extern GlobalProperty hw_compat_rhel_8_0[];
+extern const size_t hw_compat_rhel_8_0_len;
+
+extern GlobalProperty hw_compat_rhel_7_6[];
+extern const size_t hw_compat_rhel_7_6_len;
+
+extern GlobalProperty hw_compat_rhel_7_5[];
+extern const size_t hw_compat_rhel_7_5_len;
+
+extern GlobalProperty hw_compat_rhel_7_4[];
+extern const size_t hw_compat_rhel_7_4_len;
+
+extern GlobalProperty hw_compat_rhel_7_3[];
+extern const size_t hw_compat_rhel_7_3_len;
+
+extern GlobalProperty hw_compat_rhel_7_2[];
+extern const size_t hw_compat_rhel_7_2_len;
+
+extern GlobalProperty hw_compat_rhel_7_1[];
+extern const size_t hw_compat_rhel_7_1_len;
+
 #endif
diff --git a/include/hw/usb.h b/include/hw/usb.h
index c24d968a19..b353438ea0 100644
--- a/include/hw/usb.h
+++ b/include/hw/usb.h
@@ -605,4 +605,8 @@ int usb_get_quirks(uint16_t vendor_id, uint16_t product_id,
                    uint8_t interface_class, uint8_t interface_subclass,
                    uint8_t interface_protocol);
 
+
+/* hcd-xhci.c -- rhel7.0.0 machine type compatibility */
+extern bool migrate_cve_2014_5263_xhci_fields;
+
 #endif
diff --git a/migration/migration.c b/migration/migration.c
index 354ad072fa..30c53c623b 100644
--- a/migration/migration.c
+++ b/migration/migration.c
@@ -121,6 +121,8 @@ enum mig_rp_message_type {
     MIG_RP_MSG_MAX
 };
 
+bool migrate_pre_2_2;
+
 /* When we add fault tolerance, we could have several
    migrations at once.  For now we don't need to add
    dynamic creation of migration */
diff --git a/migration/migration.h b/migration/migration.h
index 79b3dda146..0b1b0d4df5 100644
--- a/migration/migration.h
+++ b/migration/migration.h
@@ -335,6 +335,11 @@ void init_dirty_bitmap_incoming_migration(void);
 void migrate_add_address(SocketAddress *address);
 
 int foreach_not_ignored_block(RAMBlockIterFunc func, void *opaque);
+/*
+ * Disables a load of subsections that were added in 2.2/rh7.2 for backwards
+ * migration compatibility.
+ */
+extern bool migrate_pre_2_2;
 
 #define qemu_ram_foreach_block \
   #warning "Use foreach_not_ignored_block in migration code"
-- 
2.21.0

