From adf66c037e60d66f864960b24c746b767efb10b9 Mon Sep 17 00:00:00 2001
From: Thomas Huth <thuth@redhat.com>
Date: Wed, 11 Nov 2020 12:03:10 -0500
Subject: [PATCH 10/18] s390/sclp: use cpu offset to locate cpu entries

RH-Author: Thomas Huth <thuth@redhat.com>
Message-id: <20201111120316.707489-7-thuth@redhat.com>
Patchwork-id: 99503
O-Subject: [RHEL-8.4.0 qemu-kvm PATCH v2 06/12] s390/sclp: use cpu offset to locate cpu entries
Bugzilla: 1798506
RH-Acked-by: Jens Freimann <jfreimann@redhat.com>
RH-Acked-by: Cornelia Huck <cohuck@redhat.com>
RH-Acked-by: David Hildenbrand <david@redhat.com>

From: Collin Walling <walling@linux.ibm.com>

The start of the CPU entry region in the Read SCP Info response data is
denoted by the offset_cpu field. As such, QEMU needs to begin creating
entries at this address.

This is in preparation for when Read SCP Info inevitably introduces new
bytes that push the start of the CPUEntry field further away.

Read CPU Info is unlikely to ever change, so let's not bother
accounting for the offset there.

Signed-off-by: Collin Walling <walling@linux.ibm.com>
Reviewed-by: Thomas Huth <thuth@redhat.com>
Reviewed-by: Cornelia Huck <cohuck@redhat.com>
Reviewed-by: Claudio Imbrenda <imbrenda@linux.ibm.com>
Message-Id: <20200915194416.107460-6-walling@linux.ibm.com>
Signed-off-by: Cornelia Huck <cohuck@redhat.com>
(cherry picked from commit 1a7a568859473b1cda39a015493c5c82bb200281)
Signed-off-by: Thomas Huth <thuth@redhat.com>
Signed-off-by: Danilo C. L. de Paula <ddepaula@redhat.com>
---
 hw/s390x/sclp.c | 6 ++++--
 1 file changed, 4 insertions(+), 2 deletions(-)

diff --git a/hw/s390x/sclp.c b/hw/s390x/sclp.c
index 2b4c6c5cfad..017989b3888 100644
--- a/hw/s390x/sclp.c
+++ b/hw/s390x/sclp.c
@@ -89,6 +89,8 @@ static void read_SCP_info(SCLPDevice *sclp, SCCB *sccb)
     int rnsize, rnmax;
     IplParameterBlock *ipib = s390_ipl_get_iplb();
     int required_len = SCCB_REQ_LEN(ReadInfo, machine->possible_cpus->len);
+    int offset_cpu = offsetof(ReadInfo, entries);
+    CPUEntry *entries_start = (void *)sccb + offset_cpu;
 
     if (be16_to_cpu(sccb->h.length) < required_len) {
         sccb->h.response_code = cpu_to_be16(SCLP_RC_INSUFFICIENT_SCCB_LENGTH);
@@ -96,9 +98,9 @@ static void read_SCP_info(SCLPDevice *sclp, SCCB *sccb)
     }
 
     /* CPU information */
-    prepare_cpu_entries(machine, read_info->entries, &cpu_count);
+    prepare_cpu_entries(machine, entries_start, &cpu_count);
     read_info->entries_cpu = cpu_to_be16(cpu_count);
-    read_info->offset_cpu = cpu_to_be16(offsetof(ReadInfo, entries));
+    read_info->offset_cpu = cpu_to_be16(offset_cpu);
     read_info->highest_cpu = cpu_to_be16(machine->smp.max_cpus - 1);
 
     read_info->ibc_val = cpu_to_be32(s390_get_ibc_val());
-- 
2.27.0

