From e1a3684f9b08fa9db35331b5c5ad11879f512e90 Mon Sep 17 00:00:00 2001
From: Thomas Huth <thuth@redhat.com>
Date: Wed, 11 Nov 2020 12:03:11 -0500
Subject: [PATCH 11/18] s390/sclp: add extended-length sccb support for kvm
 guest

RH-Author: Thomas Huth <thuth@redhat.com>
Message-id: <20201111120316.707489-8-thuth@redhat.com>
Patchwork-id: 99504
O-Subject: [RHEL-8.4.0 qemu-kvm PATCH v2 07/12] s390/sclp: add extended-length sccb support for kvm guest
Bugzilla: 1798506
RH-Acked-by: Jens Freimann <jfreimann@redhat.com>
RH-Acked-by: Cornelia Huck <cohuck@redhat.com>
RH-Acked-by: David Hildenbrand <david@redhat.com>

From: Collin Walling <walling@linux.ibm.com>

As more features and facilities are added to the Read SCP Info (RSCPI)
response, more space is required to store them. The space used to store
these new features intrudes on the space originally used to store CPU
entries. This means as more features and facilities are added to the
RSCPI response, less space can be used to store CPU entries.

With the Extended-Length SCCB (ELS) facility, a KVM guest can execute
the RSCPI command and determine if the SCCB is large enough to store a
complete reponse. If it is not large enough, then the required length
will be set in the SCCB header.

The caller of the SCLP command is responsible for creating a
large-enough SCCB to store a complete response. Proper checking should
be in place, and the caller should execute the command once-more with
the large-enough SCCB.

This facility also enables an extended SCCB for the Read CPU Info
(RCPUI) command.

When this facility is enabled, the boundary violation response cannot
be a result from the RSCPI, RSCPI Forced, or RCPUI commands.

In order to tolerate kernels that do not yet have full support for this
feature, a "fixed" offset to the start of the CPU Entries within the
Read SCP Info struct is set to allow for the original 248 max entries
when this feature is disabled.

Additionally, this is introduced as a CPU feature to protect the guest
from migrating to a machine that does not support storing an extended
SCCB. This could otherwise hinder the VM from being able to read all
available CPU entries after migration (such as during re-ipl).

Signed-off-by: Collin Walling <walling@linux.ibm.com>
Reviewed-by: Thomas Huth <thuth@redhat.com>
Acked-by: Cornelia Huck <cohuck@redhat.com>
Reviewed-by: Claudio Imbrenda <imbrenda@linux.ibm.com>
Message-Id: <20200915194416.107460-7-walling@linux.ibm.com>
Signed-off-by: Cornelia Huck <cohuck@redhat.com>
(cherry picked from commit 1ecd6078f587cfadda8edc93d45b5072e35f2d17)
Signed-off-by: Thomas Huth <thuth@redhat.com>
Signed-off-by: Danilo C. L. de Paula <ddepaula@redhat.com>
---
 hw/s390x/sclp.c                     | 43 +++++++++++++++++++++++++----
 include/hw/s390x/sclp.h             |  1 +
 target/s390x/cpu_features_def.inc.h |  1 +
 target/s390x/gen-features.c         |  1 +
 target/s390x/kvm.c                  |  8 ++++++
 5 files changed, 48 insertions(+), 6 deletions(-)

diff --git a/hw/s390x/sclp.c b/hw/s390x/sclp.c
index 017989b3888..8d111628e04 100644
--- a/hw/s390x/sclp.c
+++ b/hw/s390x/sclp.c
@@ -49,13 +49,30 @@ static inline bool sclp_command_code_valid(uint32_t code)
     return false;
 }
 
-static bool sccb_verify_boundary(uint64_t sccb_addr, uint16_t sccb_len)
+static bool sccb_verify_boundary(uint64_t sccb_addr, uint16_t sccb_len,
+                                 uint32_t code)
 {
     uint64_t sccb_max_addr = sccb_addr + sccb_len - 1;
     uint64_t sccb_boundary = (sccb_addr & PAGE_MASK) + PAGE_SIZE;
 
-    if (sccb_max_addr < sccb_boundary) {
-        return true;
+    switch (code & SCLP_CMD_CODE_MASK) {
+    case SCLP_CMDW_READ_SCP_INFO:
+    case SCLP_CMDW_READ_SCP_INFO_FORCED:
+    case SCLP_CMDW_READ_CPU_INFO:
+        /*
+         * An extended-length SCCB is only allowed for Read SCP/CPU Info and
+         * is allowed to exceed the 4k boundary. The respective commands will
+         * set the length field to the required length if an insufficient
+         * SCCB length is provided.
+         */
+        if (s390_has_feat(S390_FEAT_EXTENDED_LENGTH_SCCB)) {
+            return true;
+        }
+        /* fallthrough */
+    default:
+        if (sccb_max_addr < sccb_boundary) {
+            return true;
+        }
     }
 
     return false;
@@ -80,6 +97,12 @@ static void prepare_cpu_entries(MachineState *ms, CPUEntry *entry, int *count)
 
 #define SCCB_REQ_LEN(s, max_cpus) (sizeof(s) + max_cpus * sizeof(CPUEntry))
 
+static inline bool ext_len_sccb_supported(SCCBHeader header)
+{
+    return s390_has_feat(S390_FEAT_EXTENDED_LENGTH_SCCB) &&
+           header.control_mask[2] & SCLP_VARIABLE_LENGTH_RESPONSE;
+}
+
 /* Provide information about the configuration, CPUs and storage */
 static void read_SCP_info(SCLPDevice *sclp, SCCB *sccb)
 {
@@ -89,10 +112,15 @@ static void read_SCP_info(SCLPDevice *sclp, SCCB *sccb)
     int rnsize, rnmax;
     IplParameterBlock *ipib = s390_ipl_get_iplb();
     int required_len = SCCB_REQ_LEN(ReadInfo, machine->possible_cpus->len);
-    int offset_cpu = offsetof(ReadInfo, entries);
+    int offset_cpu = s390_has_feat(S390_FEAT_EXTENDED_LENGTH_SCCB) ?
+                     offsetof(ReadInfo, entries) :
+                     SCLP_READ_SCP_INFO_FIXED_CPU_OFFSET;
     CPUEntry *entries_start = (void *)sccb + offset_cpu;
 
     if (be16_to_cpu(sccb->h.length) < required_len) {
+        if (ext_len_sccb_supported(sccb->h)) {
+            sccb->h.length = cpu_to_be16(required_len);
+        }
         sccb->h.response_code = cpu_to_be16(SCLP_RC_INSUFFICIENT_SCCB_LENGTH);
         return;
     }
@@ -153,6 +181,9 @@ static void sclp_read_cpu_info(SCLPDevice *sclp, SCCB *sccb)
     int required_len = SCCB_REQ_LEN(ReadCpuInfo, machine->possible_cpus->len);
 
     if (be16_to_cpu(sccb->h.length) < required_len) {
+        if (ext_len_sccb_supported(sccb->h)) {
+            sccb->h.length = cpu_to_be16(required_len);
+        }
         sccb->h.response_code = cpu_to_be16(SCLP_RC_INSUFFICIENT_SCCB_LENGTH);
         return;
     }
@@ -249,7 +280,7 @@ int sclp_service_call_protected(CPUS390XState *env, uint64_t sccb,
         goto out_write;
     }
 
-    if (!sccb_verify_boundary(sccb, be16_to_cpu(work_sccb->h.length))) {
+    if (!sccb_verify_boundary(sccb, be16_to_cpu(work_sccb->h.length), code)) {
         work_sccb->h.response_code = cpu_to_be16(SCLP_RC_SCCB_BOUNDARY_VIOLATION);
         goto out_write;
     }
@@ -302,7 +333,7 @@ int sclp_service_call(CPUS390XState *env, uint64_t sccb, uint32_t code)
         goto out_write;
     }
 
-    if (!sccb_verify_boundary(sccb, be16_to_cpu(work_sccb->h.length))) {
+    if (!sccb_verify_boundary(sccb, be16_to_cpu(work_sccb->h.length), code)) {
         work_sccb->h.response_code = cpu_to_be16(SCLP_RC_SCCB_BOUNDARY_VIOLATION);
         goto out_write;
     }
diff --git a/include/hw/s390x/sclp.h b/include/hw/s390x/sclp.h
index 55f53a46540..df2fa4169b0 100644
--- a/include/hw/s390x/sclp.h
+++ b/include/hw/s390x/sclp.h
@@ -110,6 +110,7 @@ typedef struct CPUEntry {
     uint8_t reserved1;
 } QEMU_PACKED CPUEntry;
 
+#define SCLP_READ_SCP_INFO_FIXED_CPU_OFFSET     128
 typedef struct ReadInfo {
     SCCBHeader h;
     uint16_t rnmax;
diff --git a/target/s390x/cpu_features_def.inc.h b/target/s390x/cpu_features_def.inc.h
index 60db28351d0..3548d65a69a 100644
--- a/target/s390x/cpu_features_def.inc.h
+++ b/target/s390x/cpu_features_def.inc.h
@@ -97,6 +97,7 @@ DEF_FEAT(GUARDED_STORAGE, "gs", STFL, 133, "Guarded-storage facility")
 DEF_FEAT(VECTOR_PACKED_DECIMAL, "vxpd", STFL, 134, "Vector packed decimal facility")
 DEF_FEAT(VECTOR_ENH, "vxeh", STFL, 135, "Vector enhancements facility")
 DEF_FEAT(MULTIPLE_EPOCH, "mepoch", STFL, 139, "Multiple-epoch facility")
+DEF_FEAT(EXTENDED_LENGTH_SCCB, "els", STFL, 140, "Extended-length SCCB facility")
 DEF_FEAT(TEST_PENDING_EXT_INTERRUPTION, "tpei", STFL, 144, "Test-pending-external-interruption facility")
 DEF_FEAT(INSERT_REFERENCE_BITS_MULT, "irbm", STFL, 145, "Insert-reference-bits-multiple facility")
 DEF_FEAT(MSA_EXT_8, "msa8-base", STFL, 146, "Message-security-assist-extension-8 facility (excluding subfunctions)")
diff --git a/target/s390x/gen-features.c b/target/s390x/gen-features.c
index 8ddeebc5441..6857f657fba 100644
--- a/target/s390x/gen-features.c
+++ b/target/s390x/gen-features.c
@@ -522,6 +522,7 @@ static uint16_t full_GEN12_GA1[] = {
     S390_FEAT_AP_QUEUE_INTERRUPT_CONTROL,
     S390_FEAT_AP_FACILITIES_TEST,
     S390_FEAT_AP,
+    S390_FEAT_EXTENDED_LENGTH_SCCB,
 };
 
 static uint16_t full_GEN12_GA2[] = {
diff --git a/target/s390x/kvm.c b/target/s390x/kvm.c
index 0bbf8f81b09..ef437acb5c1 100644
--- a/target/s390x/kvm.c
+++ b/target/s390x/kvm.c
@@ -2441,6 +2441,14 @@ void kvm_s390_get_host_cpu_model(S390CPUModel *model, Error **errp)
         KVM_S390_VM_CRYPTO_ENABLE_APIE)) {
         set_bit(S390_FEAT_AP, model->features);
     }
+
+    /*
+     * Extended-Length SCCB is handled entirely within QEMU.
+     * For PV guests this is completely fenced by the Ultravisor, as Service
+     * Call error checking and STFLE interpretation are handled via SIE.
+     */
+    set_bit(S390_FEAT_EXTENDED_LENGTH_SCCB, model->features);
+
     /* strip of features that are not part of the maximum model */
     bitmap_and(model->features, model->features, model->def->full_feat,
                S390_FEAT_MAX);
-- 
2.27.0

