From db6a782f8b9ba062f195ff504b4d2f93e471fecc Mon Sep 17 00:00:00 2001
From: Thomas Huth <thuth@redhat.com>
Date: Tue, 11 May 2021 11:24:05 -0400
Subject: [PATCH 2/5] vfio-ccw: Connect the device request notifier

RH-Author: Thomas Huth <thuth@redhat.com>
Message-id: <20210511112405.297037-3-thuth@redhat.com>
Patchwork-id: 101536
O-Subject: [RHEL-8.5.0 qemu-kvm PATCH 2/2] vfio-ccw: Connect the device request notifier
Bugzilla: 1940450
RH-Acked-by: Laszlo Ersek <lersek@redhat.com>
RH-Acked-by: Cornelia Huck <cohuck@redhat.com>
RH-Acked-by: David Hildenbrand <david@redhat.com>

Now that the vfio-ccw code has a notifier interface to request that
a device be unplugged, let's wire that together.

Signed-off-by: Eric Farman <farman@linux.ibm.com>
Reviewed-by: Cornelia Huck <cohuck@redhat.com>
Message-Id: <20210104202057.48048-4-farman@linux.ibm.com>
Signed-off-by: Cornelia Huck <cohuck@redhat.com>
(cherry picked from commit b2f96f9e4f5fbc8f2770a436191cb328da4d5350)
Bugzilla: https://bugzilla.redhat.com/show_bug.cgi?id=1940450
Signed-off-by: Thomas Huth <thuth@redhat.com>
Signed-off-by: Danilo C. L. de Paula <ddepaula@redhat.com>
---
 hw/vfio/ccw.c | 40 ++++++++++++++++++++++++++++++++++++----
 1 file changed, 36 insertions(+), 4 deletions(-)

diff --git a/hw/vfio/ccw.c b/hw/vfio/ccw.c
index b72a505893..3d450fe1c9 100644
--- a/hw/vfio/ccw.c
+++ b/hw/vfio/ccw.c
@@ -49,6 +49,7 @@ struct VFIOCCWDevice {
     struct ccw_crw_region *crw_region;
     EventNotifier io_notifier;
     EventNotifier crw_notifier;
+    EventNotifier req_notifier;
     bool force_orb_pfch;
     bool warned_orb_pfch;
 };
@@ -287,6 +288,21 @@ static void vfio_ccw_crw_read(VFIOCCWDevice *vcdev)
     } while (1);
 }
 
+static void vfio_ccw_req_notifier_handler(void *opaque)
+{
+    VFIOCCWDevice *vcdev = opaque;
+    Error *err = NULL;
+
+    if (!event_notifier_test_and_clear(&vcdev->req_notifier)) {
+        return;
+    }
+
+    qdev_unplug(DEVICE(vcdev), &err);
+    if (err) {
+        warn_reportf_err(err, VFIO_MSG_PREFIX, vcdev->vdev.name);
+    }
+}
+
 static void vfio_ccw_crw_notifier_handler(void *opaque)
 {
     VFIOCCWDevice *vcdev = opaque;
@@ -386,6 +402,10 @@ static void vfio_ccw_register_irq_notifier(VFIOCCWDevice *vcdev,
         notifier = &vcdev->crw_notifier;
         fd_read = vfio_ccw_crw_notifier_handler;
         break;
+    case VFIO_CCW_REQ_IRQ_INDEX:
+        notifier = &vcdev->req_notifier;
+        fd_read = vfio_ccw_req_notifier_handler;
+        break;
     default:
         error_setg(errp, "vfio: Unsupported device irq(%d)", irq);
         return;
@@ -440,6 +460,9 @@ static void vfio_ccw_unregister_irq_notifier(VFIOCCWDevice *vcdev,
     case VFIO_CCW_CRW_IRQ_INDEX:
         notifier = &vcdev->crw_notifier;
         break;
+    case VFIO_CCW_REQ_IRQ_INDEX:
+        notifier = &vcdev->req_notifier;
+        break;
     default:
         error_report("vfio: Unsupported device irq(%d)", irq);
         return;
@@ -657,20 +680,28 @@ static void vfio_ccw_realize(DeviceState *dev, Error **errp)
 
     vfio_ccw_register_irq_notifier(vcdev, VFIO_CCW_IO_IRQ_INDEX, &err);
     if (err) {
-        goto out_notifier_err;
+        goto out_io_notifier_err;
     }
 
     if (vcdev->crw_region) {
         vfio_ccw_register_irq_notifier(vcdev, VFIO_CCW_CRW_IRQ_INDEX, &err);
         if (err) {
-            vfio_ccw_unregister_irq_notifier(vcdev, VFIO_CCW_IO_IRQ_INDEX);
-            goto out_notifier_err;
+            goto out_crw_notifier_err;
         }
     }
 
+    vfio_ccw_register_irq_notifier(vcdev, VFIO_CCW_REQ_IRQ_INDEX, &err);
+    if (err) {
+        goto out_req_notifier_err;
+    }
+
     return;
 
-out_notifier_err:
+out_req_notifier_err:
+    vfio_ccw_unregister_irq_notifier(vcdev, VFIO_CCW_CRW_IRQ_INDEX);
+out_crw_notifier_err:
+    vfio_ccw_unregister_irq_notifier(vcdev, VFIO_CCW_IO_IRQ_INDEX);
+out_io_notifier_err:
     vfio_ccw_put_region(vcdev);
 out_region_err:
     vfio_ccw_put_device(vcdev);
@@ -692,6 +723,7 @@ static void vfio_ccw_unrealize(DeviceState *dev, Error **errp)
     S390CCWDeviceClass *cdc = S390_CCW_DEVICE_GET_CLASS(cdev);
     VFIOGroup *group = vcdev->vdev.group;
 
+    vfio_ccw_unregister_irq_notifier(vcdev, VFIO_CCW_REQ_IRQ_INDEX);
     vfio_ccw_unregister_irq_notifier(vcdev, VFIO_CCW_CRW_IRQ_INDEX);
     vfio_ccw_unregister_irq_notifier(vcdev, VFIO_CCW_IO_IRQ_INDEX);
     vfio_ccw_put_region(vcdev);
-- 
2.27.0

