From d9a63d12b5804eb172a040a16d7e725853c41a8c Mon Sep 17 00:00:00 2001
From: Thomas Huth <thuth@redhat.com>
Date: Wed, 11 Nov 2020 12:03:12 -0500
Subject: [PATCH 12/18] linux-headers: Partial update against Linux 5.9-rc4

RH-Author: Thomas Huth <thuth@redhat.com>
Message-id: <20201111120316.707489-9-thuth@redhat.com>
Patchwork-id: 99505
O-Subject: [RHEL-8.4.0 qemu-kvm PATCH v2 08/12] linux-headers: Partial update against Linux 5.9-rc4
Bugzilla: 1798506
RH-Acked-by: Jens Freimann <jfreimann@redhat.com>
RH-Acked-by: Cornelia Huck <cohuck@redhat.com>
RH-Acked-by: David Hildenbrand <david@redhat.com>

Upstream-status: N/A

This is based on upstream commit e6546342a830e520d14ef03aa95677611de0d90c
but only the two files have been included (there were too many conflicts
in the other unrelated files, so they have been dropped from this patch).

Signed-off-by: Thomas Huth <thuth@redhat.com>
Signed-off-by: Danilo C. L. de Paula <ddepaula@redhat.com>
---
 linux-headers/asm-s390/kvm.h | 7 +++++--
 linux-headers/linux/kvm.h    | 6 ++++++
 2 files changed, 11 insertions(+), 2 deletions(-)

diff --git a/linux-headers/asm-s390/kvm.h b/linux-headers/asm-s390/kvm.h
index 0138ccb0d89..f053b8304a8 100644
--- a/linux-headers/asm-s390/kvm.h
+++ b/linux-headers/asm-s390/kvm.h
@@ -231,11 +231,13 @@ struct kvm_guest_debug_arch {
 #define KVM_SYNC_GSCB   (1UL << 9)
 #define KVM_SYNC_BPBC   (1UL << 10)
 #define KVM_SYNC_ETOKEN (1UL << 11)
+#define KVM_SYNC_DIAG318 (1UL << 12)
 
 #define KVM_SYNC_S390_VALID_FIELDS \
 	(KVM_SYNC_PREFIX | KVM_SYNC_GPRS | KVM_SYNC_ACRS | KVM_SYNC_CRS | \
 	 KVM_SYNC_ARCH0 | KVM_SYNC_PFAULT | KVM_SYNC_VRS | KVM_SYNC_RICCB | \
-	 KVM_SYNC_FPRS | KVM_SYNC_GSCB | KVM_SYNC_BPBC | KVM_SYNC_ETOKEN)
+	 KVM_SYNC_FPRS | KVM_SYNC_GSCB | KVM_SYNC_BPBC | KVM_SYNC_ETOKEN | \
+	 KVM_SYNC_DIAG318)
 
 /* length and alignment of the sdnx as a power of two */
 #define SDNXC 8
@@ -264,7 +266,8 @@ struct kvm_sync_regs {
 	__u8 reserved2 : 7;
 	__u8 padding1[51];	/* riccb needs to be 64byte aligned */
 	__u8 riccb[64];		/* runtime instrumentation controls block */
-	__u8 padding2[192];	/* sdnx needs to be 256byte aligned */
+	__u64 diag318;		/* diagnose 0x318 info */
+	__u8 padding2[184];	/* sdnx needs to be 256byte aligned */
 	union {
 		__u8 sdnx[SDNXL];  /* state description annex */
 		struct {
diff --git a/linux-headers/linux/kvm.h b/linux-headers/linux/kvm.h
index 578cd97c0d9..6bba4ec136b 100644
--- a/linux-headers/linux/kvm.h
+++ b/linux-headers/linux/kvm.h
@@ -276,6 +276,7 @@ struct kvm_run {
 		/* KVM_EXIT_FAIL_ENTRY */
 		struct {
 			__u64 hardware_entry_failure_reason;
+			__u32 cpu;
 		} fail_entry;
 		/* KVM_EXIT_EXCEPTION */
 		struct {
@@ -1011,6 +1012,11 @@ struct kvm_ppc_resize_hpt {
 #define KVM_CAP_S390_VCPU_RESETS 179
 #define KVM_CAP_S390_PROTECTED 180
 #define KVM_CAP_PPC_SECURE_GUEST 181
+#define KVM_CAP_HALT_POLL 182
+#define KVM_CAP_ASYNC_PF_INT 183
+#define KVM_CAP_LAST_CPU 184
+#define KVM_CAP_SMALLER_MAXPHYADDR 185
+#define KVM_CAP_S390_DIAG318 186
 
 #ifdef KVM_CAP_IRQ_ROUTING
 
-- 
2.27.0

