From 70f8bbb27f9f357ea83ff6639fc00aa60fc902b9 Mon Sep 17 00:00:00 2001
From: "plai@redhat.com" <plai@redhat.com>
Date: Thu, 21 May 2020 23:56:47 +0100
Subject: [PATCH 04/12] numa: Extend CLI to provide initiator information for
 numa nodes

RH-Author: plai@redhat.com
Message-id: <20200521235655.27141-4-plai@redhat.com>
Patchwork-id: 96736
O-Subject: [RHEL8.2.1 AV qemu-kvm PATCH 03/11] numa: Extend CLI to provide initiator information for numa nodes
Bugzilla: 1600217
RH-Acked-by: Michael S. Tsirkin <mst@redhat.com>
RH-Acked-by: Igor Mammedov <imammedo@redhat.com>
RH-Acked-by: Eduardo Habkost <ehabkost@redhat.com>

From: Tao Xu <tao3.xu@intel.com>

In ACPI 6.3 chapter 5.2.27 Heterogeneous Memory Attribute Table (HMAT),
The initiator represents processor which access to memory. And in 5.2.27.3
Memory Proximity Domain Attributes Structure, the attached initiator is
defined as where the memory controller responsible for a memory proximity
domain. With attached initiator information, the topology of heterogeneous
memory can be described. Add new machine property 'hmat' to enable all
HMAT specific options.

Extend CLI of "-numa node" option to indicate the initiator numa node-id.
In the linux kernel, the codes in drivers/acpi/hmat/hmat.c parse and report
the platform's HMAT tables. Before using initiator option, enable HMAT with
-machine hmat=on.

Acked-by: Markus Armbruster <armbru@redhat.com>
Reviewed-by: Igor Mammedov <imammedo@redhat.com>
Reviewed-by: Jingqi Liu <jingqi.liu@intel.com>
Suggested-by: Dan Williams <dan.j.williams@intel.com>
Signed-off-by: Tao Xu <tao3.xu@intel.com>
Message-Id: <20191213011929.2520-2-tao3.xu@intel.com>
Reviewed-by: Michael S. Tsirkin <mst@redhat.com>
Signed-off-by: Michael S. Tsirkin <mst@redhat.com>
(cherry picked from commit 244b3f4485a07c7ce4b7123d6ce9d8c6012756e8)
Signed-off-by: Paul Lai <plai@redhat.com>
Signed-off-by: Danilo C. L. de Paula <ddepaula@redhat.com>
---
 hw/core/machine.c     | 64 +++++++++++++++++++++++++++++++++++++++++++++++++++
 hw/core/numa.c        | 23 ++++++++++++++++++
 include/sysemu/numa.h |  5 ++++
 qapi/machine.json     | 10 +++++++-
 qemu-options.hx       | 35 ++++++++++++++++++++++++----
 5 files changed, 131 insertions(+), 6 deletions(-)

diff --git a/hw/core/machine.c b/hw/core/machine.c
index 19c78c6..cb21ae1 100644
--- a/hw/core/machine.c
+++ b/hw/core/machine.c
@@ -688,6 +688,20 @@ static void machine_set_nvdimm(Object *obj, bool value, Error **errp)
     ms->nvdimms_state->is_enabled = value;
 }
 
+static bool machine_get_hmat(Object *obj, Error **errp)
+{
+    MachineState *ms = MACHINE(obj);
+
+    return ms->numa_state->hmat_enabled;
+}
+
+static void machine_set_hmat(Object *obj, bool value, Error **errp)
+{
+    MachineState *ms = MACHINE(obj);
+
+    ms->numa_state->hmat_enabled = value;
+}
+
 static char *machine_get_nvdimm_persistence(Object *obj, Error **errp)
 {
     MachineState *ms = MACHINE(obj);
@@ -815,6 +829,7 @@ void machine_set_cpu_numa_node(MachineState *machine,
                                const CpuInstanceProperties *props, Error **errp)
 {
     MachineClass *mc = MACHINE_GET_CLASS(machine);
+    NodeInfo *numa_info = machine->numa_state->nodes;
     bool match = false;
     int i;
 
@@ -884,6 +899,17 @@ void machine_set_cpu_numa_node(MachineState *machine,
         match = true;
         slot->props.node_id = props->node_id;
         slot->props.has_node_id = props->has_node_id;
+
+        if (machine->numa_state->hmat_enabled) {
+            if ((numa_info[props->node_id].initiator < MAX_NODES) &&
+                (props->node_id != numa_info[props->node_id].initiator)) {
+                error_setg(errp, "The initiator of CPU NUMA node %" PRId64
+                        " should be itself", props->node_id);
+                return;
+            }
+            numa_info[props->node_id].has_cpu = true;
+            numa_info[props->node_id].initiator = props->node_id;
+        }
     }
 
     if (!match) {
@@ -1130,6 +1156,13 @@ static void machine_initfn(Object *obj)
 
     if (mc->cpu_index_to_instance_props && mc->get_default_cpu_node_id) {
         ms->numa_state = g_new0(NumaState, 1);
+        object_property_add_bool(obj, "hmat",
+                                 machine_get_hmat, machine_set_hmat,
+                                 &error_abort);
+        object_property_set_description(obj, "hmat",
+                                        "Set on/off to enable/disable "
+                                        "ACPI Heterogeneous Memory Attribute "
+                                        "Table (HMAT)", NULL);
     }
 
     /* Register notifier when init is done for sysbus sanity checks */
@@ -1218,6 +1251,32 @@ static char *cpu_slot_to_string(const CPUArchId *cpu)
     return g_string_free(s, false);
 }
 
+static void numa_validate_initiator(NumaState *numa_state)
+{
+    int i;
+    NodeInfo *numa_info = numa_state->nodes;
+
+    for (i = 0; i < numa_state->num_nodes; i++) {
+        if (numa_info[i].initiator == MAX_NODES) {
+            error_report("The initiator of NUMA node %d is missing, use "
+                         "'-numa node,initiator' option to declare it", i);
+            exit(1);
+        }
+
+        if (!numa_info[numa_info[i].initiator].present) {
+            error_report("NUMA node %" PRIu16 " is missing, use "
+                         "'-numa node' option to declare it first",
+                         numa_info[i].initiator);
+            exit(1);
+        }
+
+        if (!numa_info[numa_info[i].initiator].has_cpu) {
+            error_report("The initiator of NUMA node %d is invalid", i);
+            exit(1);
+        }
+    }
+}
+
 static void machine_numa_finish_cpu_init(MachineState *machine)
 {
     int i;
@@ -1258,6 +1317,11 @@ static void machine_numa_finish_cpu_init(MachineState *machine)
             machine_set_cpu_numa_node(machine, &props, &error_fatal);
         }
     }
+
+    if (machine->numa_state->hmat_enabled) {
+        numa_validate_initiator(machine->numa_state);
+    }
+
     if (s->len && !qtest_enabled()) {
         warn_report("CPU(s) not present in any NUMA nodes: %s",
                     s->str);
diff --git a/hw/core/numa.c b/hw/core/numa.c
index 19f082d..a07eef9 100644
--- a/hw/core/numa.c
+++ b/hw/core/numa.c
@@ -129,6 +129,29 @@ static void parse_numa_node(MachineState *ms, NumaNodeOptions *node,
         numa_info[nodenr].node_mem = object_property_get_uint(o, "size", NULL);
         numa_info[nodenr].node_memdev = MEMORY_BACKEND(o);
     }
+
+    /*
+     * If not set the initiator, set it to MAX_NODES. And if
+     * HMAT is enabled and this node has no cpus, QEMU will raise error.
+     */
+    numa_info[nodenr].initiator = MAX_NODES;
+    if (node->has_initiator) {
+        if (!ms->numa_state->hmat_enabled) {
+            error_setg(errp, "ACPI Heterogeneous Memory Attribute Table "
+                       "(HMAT) is disabled, enable it with -machine hmat=on "
+                       "before using any of hmat specific options");
+            return;
+        }
+
+        if (node->initiator >= MAX_NODES) {
+            error_report("The initiator id %" PRIu16 " expects an integer "
+                         "between 0 and %d", node->initiator,
+                         MAX_NODES - 1);
+            return;
+        }
+
+        numa_info[nodenr].initiator = node->initiator;
+    }
     numa_info[nodenr].present = true;
     max_numa_nodeid = MAX(max_numa_nodeid, nodenr + 1);
     ms->numa_state->num_nodes++;
diff --git a/include/sysemu/numa.h b/include/sysemu/numa.h
index ae9c41d..788cbec 100644
--- a/include/sysemu/numa.h
+++ b/include/sysemu/numa.h
@@ -18,6 +18,8 @@ struct NodeInfo {
     uint64_t node_mem;
     struct HostMemoryBackend *node_memdev;
     bool present;
+    bool has_cpu;
+    uint16_t initiator;
     uint8_t distance[MAX_NODES];
 };
 
@@ -33,6 +35,9 @@ struct NumaState {
     /* Allow setting NUMA distance for different NUMA nodes */
     bool have_numa_distance;
 
+    /* Detect if HMAT support is enabled. */
+    bool hmat_enabled;
+
     /* NUMA nodes information */
     NodeInfo nodes[MAX_NODES];
 };
diff --git a/qapi/machine.json b/qapi/machine.json
index ca26779..27d0e37 100644
--- a/qapi/machine.json
+++ b/qapi/machine.json
@@ -463,6 +463,13 @@
 # @memdev: memory backend object.  If specified for one node,
 #          it must be specified for all nodes.
 #
+# @initiator: defined in ACPI 6.3 Chapter 5.2.27.3 Table 5-145,
+#             points to the nodeid which has the memory controller
+#             responsible for this NUMA node. This field provides
+#             additional information as to the initiator node that
+#             is closest (as in directly attached) to this node, and
+#             therefore has the best performance (since 5.0)
+#
 # Since: 2.1
 ##
 { 'struct': 'NumaNodeOptions',
@@ -470,7 +477,8 @@
    '*nodeid': 'uint16',
    '*cpus':   ['uint16'],
    '*mem':    'size',
-   '*memdev': 'str' }}
+   '*memdev': 'str',
+   '*initiator': 'uint16' }}
 
 ##
 # @NumaDistOptions:
diff --git a/qemu-options.hx b/qemu-options.hx
index df1d27b..e2ce754 100644
--- a/qemu-options.hx
+++ b/qemu-options.hx
@@ -43,7 +43,8 @@ DEF("machine", HAS_ARG, QEMU_OPTION_machine, \
     "                suppress-vmdesc=on|off disables self-describing migration (default=off)\n"
     "                nvdimm=on|off controls NVDIMM support (default=off)\n"
     "                enforce-config-section=on|off enforce configuration section migration (default=off)\n"
-    "                memory-encryption=@var{} memory encryption object to use (default=none)\n",
+    "                memory-encryption=@var{} memory encryption object to use (default=none)\n"
+    "                hmat=on|off controls ACPI HMAT support (default=off)\n",
     QEMU_ARCH_ALL)
 STEXI
 @item -machine [type=]@var{name}[,prop=@var{value}[,...]]
@@ -103,6 +104,9 @@ NOTE: this parameter is deprecated. Please use @option{-global}
 @option{migration.send-configuration}=@var{on|off} instead.
 @item memory-encryption=@var{}
 Memory encryption object to use. The default is none.
+@item hmat=on|off
+Enables or disables ACPI Heterogeneous Memory Attribute Table (HMAT) support.
+The default is off.
 @end table
 ETEXI
 
@@ -161,14 +165,14 @@ If any on the three values is given, the total number of CPUs @var{n} can be omi
 ETEXI
 
 DEF("numa", HAS_ARG, QEMU_OPTION_numa,
-    "-numa node[,mem=size][,cpus=firstcpu[-lastcpu]][,nodeid=node]\n"
-    "-numa node[,memdev=id][,cpus=firstcpu[-lastcpu]][,nodeid=node]\n"
+    "-numa node[,mem=size][,cpus=firstcpu[-lastcpu]][,nodeid=node][,initiator=node]\n"
+    "-numa node[,memdev=id][,cpus=firstcpu[-lastcpu]][,nodeid=node][,initiator=node]\n"
     "-numa dist,src=source,dst=destination,val=distance\n"
     "-numa cpu,node-id=node[,socket-id=x][,core-id=y][,thread-id=z]\n",
     QEMU_ARCH_ALL)
 STEXI
-@item -numa node[,mem=@var{size}][,cpus=@var{firstcpu}[-@var{lastcpu}]][,nodeid=@var{node}]
-@itemx -numa node[,memdev=@var{id}][,cpus=@var{firstcpu}[-@var{lastcpu}]][,nodeid=@var{node}]
+@item -numa node[,mem=@var{size}][,cpus=@var{firstcpu}[-@var{lastcpu}]][,nodeid=@var{node}][,initiator=@var{initiator}]
+@itemx -numa node[,memdev=@var{id}][,cpus=@var{firstcpu}[-@var{lastcpu}]][,nodeid=@var{node}][,initiator=@var{initiator}]
 @itemx -numa dist,src=@var{source},dst=@var{destination},val=@var{distance}
 @itemx -numa cpu,node-id=@var{node}[,socket-id=@var{x}][,core-id=@var{y}][,thread-id=@var{z}]
 @findex -numa
@@ -215,6 +219,27 @@ split equally between them.
 @samp{mem} and @samp{memdev} are mutually exclusive. Furthermore,
 if one node uses @samp{memdev}, all of them have to use it.
 
+@samp{initiator} is an additional option that points to an @var{initiator}
+NUMA node that has best performance (the lowest latency or largest bandwidth)
+to this NUMA @var{node}. Note that this option can be set only when
+the machine property 'hmat' is set to 'on'.
+
+Following example creates a machine with 2 NUMA nodes, node 0 has CPU.
+node 1 has only memory, and its initiator is node 0. Note that because
+node 0 has CPU, by default the initiator of node 0 is itself and must be
+itself.
+@example
+-machine hmat=on \
+-m 2G,slots=2,maxmem=4G \
+-object memory-backend-ram,size=1G,id=m0 \
+-object memory-backend-ram,size=1G,id=m1 \
+-numa node,nodeid=0,memdev=m0 \
+-numa node,nodeid=1,memdev=m1,initiator=0 \
+-smp 2,sockets=2,maxcpus=2  \
+-numa cpu,node-id=0,socket-id=0 \
+-numa cpu,node-id=0,socket-id=1
+@end example
+
 @var{source} and @var{destination} are NUMA node IDs.
 @var{distance} is the NUMA distance from @var{source} to @var{destination}.
 The distance from a node to itself is always 10. If any pair of nodes is
-- 
1.8.3.1

