From f3e80771c921560a58c30020781fa01a54be8eb0 Mon Sep 17 00:00:00 2001
From: Cornelia Huck <cohuck@redhat.com>
Date: Tue, 23 Jun 2020 09:25:43 -0400
Subject: [PATCH 09/12] config: enable VFIO_CCW

RH-Author: Cornelia Huck <cohuck@redhat.com>
Message-id: <20200623092543.358315-10-cohuck@redhat.com>
Patchwork-id: 97699
O-Subject: [RHEL-8.3.0 qemu-kvm PATCH 9/9] config: enable VFIO_CCW
Bugzilla: 1660916
RH-Acked-by: Claudio Imbrenda <cimbrend@redhat.com>
RH-Acked-by: David Hildenbrand <david@redhat.com>
RH-Acked-by: Thomas Huth <thuth@redhat.com>

Enable vfio-ccw in RHEL builds.

Upstream: n/a

Signed-off-by: Cornelia Huck <cohuck@redhat.com>
Signed-off-by: Danilo C. L. de Paula <ddepaula@redhat.com>
---
 default-configs/s390x-rh-devices.mak | 1 +
 1 file changed, 1 insertion(+)

diff --git a/default-configs/s390x-rh-devices.mak b/default-configs/s390x-rh-devices.mak
index c3c73fe752..08a15f3e01 100644
--- a/default-configs/s390x-rh-devices.mak
+++ b/default-configs/s390x-rh-devices.mak
@@ -9,6 +9,7 @@ CONFIG_SCSI=y
 CONFIG_TERMINAL3270=y
 CONFIG_VFIO=y
 CONFIG_VFIO_AP=y
+CONFIG_VFIO_CCW=y
 CONFIG_VFIO_PCI=y
 CONFIG_VHOST_USER=y
 CONFIG_VIRTIO_CCW=y
-- 
2.27.0

