From c4ae2dbb8ee406f0a015b35fb76b3d6d131900d6 Mon Sep 17 00:00:00 2001
From: eperezma <eperezma@redhat.com>
Date: Tue, 12 Jan 2021 14:36:31 -0500
Subject: [PATCH 07/17] hw/arm/smmuv3: Introduce smmuv3_s1_range_inval() helper
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

RH-Author: eperezma <eperezma@redhat.com>
Message-id: <20210112143638.374060-7-eperezma@redhat.com>
Patchwork-id: 100599
O-Subject: [RHEL-8.4.0 qemu-kvm PATCH v2 06/13] hw/arm/smmuv3: Introduce smmuv3_s1_range_inval() helper
Bugzilla: 1843852
RH-Acked-by: Xiao Wang <jasowang@redhat.com>
RH-Acked-by: Peter Xu <peterx@redhat.com>
RH-Acked-by: Auger Eric <eric.auger@redhat.com>

From: Eric Auger <eric.auger@redhat.com>

Let's introduce an helper for S1 IOVA range invalidation.
This will be used for NH_VA and NH_VAA commands. It decodes
the same fields, trace, calls the UNMAP notifiers and
invalidate the corresponding IOTLB entries.

At the moment, we do not support 3.2 range invalidation yet.
So it reduces to a single IOVA invalidation.

Note the leaf bit now is also decoded for the CMD_TLBI_NH_VAA
command. At the moment it is only used for tracing.

Signed-off-by: Eric Auger <eric.auger@redhat.com>
Reviewed-by: Peter Maydell <peter.maydell@linaro.org>
Message-id: 20200728150815.11446-7-eric.auger@redhat.com
Signed-off-by: Peter Maydell <peter.maydell@linaro.org>
(cherry picked from commit c0f9ef70377cfcbd0fa6559d5dc729a930d71b7c)
Signed-off-by: Eugenio Pérez <eperezma@redhat.com>
Signed-off-by: Danilo C. L. de Paula <ddepaula@redhat.com>
---
 hw/arm/smmuv3.c     | 36 +++++++++++++++++-------------------
 hw/arm/trace-events |  3 +--
 2 files changed, 18 insertions(+), 21 deletions(-)

diff --git a/hw/arm/smmuv3.c b/hw/arm/smmuv3.c
index 067c9480a03..ae2b769f891 100644
--- a/hw/arm/smmuv3.c
+++ b/hw/arm/smmuv3.c
@@ -824,6 +824,22 @@ static void smmuv3_inv_notifiers_iova(SMMUState *s, int asid, dma_addr_t iova)
     }
 }
 
+static void smmuv3_s1_range_inval(SMMUState *s, Cmd *cmd)
+{
+    dma_addr_t addr = CMD_ADDR(cmd);
+    uint8_t type = CMD_TYPE(cmd);
+    uint16_t vmid = CMD_VMID(cmd);
+    bool leaf = CMD_LEAF(cmd);
+    int asid = -1;
+
+    if (type == SMMU_CMD_TLBI_NH_VA) {
+        asid = CMD_ASID(cmd);
+    }
+    trace_smmuv3_s1_range_inval(vmid, asid, addr, leaf);
+    smmuv3_inv_notifiers_iova(s, asid, addr);
+    smmu_iotlb_inv_iova(s, asid, addr);
+}
+
 static int smmuv3_cmdq_consume(SMMUv3State *s)
 {
     SMMUState *bs = ARM_SMMU(s);
@@ -954,27 +970,9 @@ static int smmuv3_cmdq_consume(SMMUv3State *s)
             smmu_iotlb_inv_all(bs);
             break;
         case SMMU_CMD_TLBI_NH_VAA:
-        {
-            dma_addr_t addr = CMD_ADDR(&cmd);
-            uint16_t vmid = CMD_VMID(&cmd);
-
-            trace_smmuv3_cmdq_tlbi_nh_vaa(vmid, addr);
-            smmuv3_inv_notifiers_iova(bs, -1, addr);
-            smmu_iotlb_inv_iova(bs, -1, addr);
-            break;
-        }
         case SMMU_CMD_TLBI_NH_VA:
-        {
-            uint16_t asid = CMD_ASID(&cmd);
-            uint16_t vmid = CMD_VMID(&cmd);
-            dma_addr_t addr = CMD_ADDR(&cmd);
-            bool leaf = CMD_LEAF(&cmd);
-
-            trace_smmuv3_cmdq_tlbi_nh_va(vmid, asid, addr, leaf);
-            smmuv3_inv_notifiers_iova(bs, asid, addr);
-            smmu_iotlb_inv_iova(bs, asid, addr);
+            smmuv3_s1_range_inval(bs, &cmd);
             break;
-        }
         case SMMU_CMD_TLBI_EL3_ALL:
         case SMMU_CMD_TLBI_EL3_VA:
         case SMMU_CMD_TLBI_EL2_ALL:
diff --git a/hw/arm/trace-events b/hw/arm/trace-events
index f74d3e920f1..c219fe9e828 100644
--- a/hw/arm/trace-events
+++ b/hw/arm/trace-events
@@ -45,8 +45,7 @@ smmuv3_cmdq_cfgi_ste_range(int start, int end) "start=0x%d - end=0x%d"
 smmuv3_cmdq_cfgi_cd(uint32_t sid) "streamid = %d"
 smmuv3_config_cache_hit(uint32_t sid, uint32_t hits, uint32_t misses, uint32_t perc) "Config cache HIT for sid %d (hits=%d, misses=%d, hit rate=%d)"
 smmuv3_config_cache_miss(uint32_t sid, uint32_t hits, uint32_t misses, uint32_t perc) "Config cache MISS for sid %d (hits=%d, misses=%d, hit rate=%d)"
-smmuv3_cmdq_tlbi_nh_va(int vmid, int asid, uint64_t addr, bool leaf) "vmid =%d asid =%d addr=0x%"PRIx64" leaf=%d"
-smmuv3_cmdq_tlbi_nh_vaa(int vmid, uint64_t addr) "vmid =%d addr=0x%"PRIx64
+smmuv3_s1_range_inval(int vmid, int asid, uint64_t addr, bool leaf) "vmid =%d asid =%d addr=0x%"PRIx64" leaf=%d"
 smmuv3_cmdq_tlbi_nh(void) ""
 smmuv3_cmdq_tlbi_nh_asid(uint16_t asid) "asid=%d"
 smmuv3_config_cache_inv(uint32_t sid) "Config cache INV for sid %d"
-- 
2.27.0

